|  |  |  |
| --- | --- | --- |
| **G:\Art, Photos, Logos, Movies, etc\logos\Hyundai_Chrome_Blue_Stacked.jpg** | Hyundai Motor America3200 Park Center Drive, Costa Mesa, CA 92867**TEL: 714-965-3000 FAX: 714-378-1008MEDIA WEBSITE: HyundaiNews.com** **CORPORATE WEBSITE: HyundaiUSA.com** | NewsBureauLogo |
| **2013 Santa Fe** |
| **ENGINE** |
|  | **Santa Fe Sport** | **Santa Fe** |
| **2.4L** | **2.0L Turbo** | **3.3L** |
| Type | 2.4L GDI DOHC 16-valve Inline 4-cylinder | 2.0L Turbo GDI DOHC 16-valve Inline 4-cylinder | 3.3L GDI DOHC 24-valve V6 |
| Materials | Aluminum block/aluminum cylinder heads | Aluminum block/aluminum cylinder heads | Aluminum block/aluminum cylinder heads |
| Bore & stroke | 88.0 mm x 97.0 mm | 86.0 mm x 86.0 mm | 92.0 mm x 83.8 mm |
| Displacement | 2.4L / 2,359 cc | 2.0 L / 1,998 cc | 3.3L / 3,342 cc |
| Horsepower | 190 @ 6,300 rpm | 264 @ 6,000 rpm | 290 @ 6,400 rpm |
| Torque | 181 lb-ft @ 4,250 rpm | 269 lb-ft @ 1,750~ 3,000 rpm | 252 lb-ft @ 5,200 rpm |
| Valves per cylinder | 4 | 4 | 4 |
| Compression Ratio | 11.3 | 9.5 | 11.5 |
| **TRANSMISSION** |
| 6-speed electronic automatic | **Santa Fe Sport** | **Santa Fe** |
| Gear ratios   | **2.4L** | **2.0T** | **3.3L** |
| First  | 4.639 | 4.651 | 4.651 |
| Second  | 2.826 | 2.831 | 2.831 |
| Third  | 1.841 | 1.842 | 1.842 |
| Fourth  | 1,386 | 1.386 | 1.386 |
| Fifth | 1.000 | 1.000 | 1.000 |
| Sixth | 0.772 | 0.772 | 0.772 |
| Reverse  | 3.385 | 3.393 | 3.393 |
| Final Gear Ratio | 3.648 | 3.510 | 3.041 |
| **TOWING** |
|  | **Santa Fe Sport** | **Santa Fe** |
| Towing Capacity (Trailer Weight) | **2.4L** | **2.0T** | **3.3L** |
| Without trailer brake | 2,000 lbs. | 3,500 lbs. | 5,000 lbs. |
| **SUSPENSION** |
| Front  | MacPherson strut with twin-tube gas filled damper and 26-mm stabilizer bar  |
| Rear  | Multi-link with gas shock absorber and (FWD 21 mm AWD 19 mm) stabilizer bar  |
| **STEERING** |
| Type | Motor Driven Power Steering (MDPS) |
| Overall Ratio  | 15.03 : 1 |
| Turns, lock to lock  | 2.95 |
| Turning circle (curb to curb)  | 35.8 ft (Santa Fe Sport), 36.9 ft (Santa Fe) |
| **BRAKES/TIRES/WHEELS** |
| Front | Ventilated single piston disc, 12.6 in. x 1.1 in. (320mm x 28mm) |
| Rear | Solid single piston disc, 11.9 in. X 0.4 in. (302mm x 11mm) |
| ABS | 4-wheel, 4-channel, 4-sensors with Electronic Brake-force Distribution (EBD) and Brake Assist |
| Wheels | 17 x 7.0 aluminum alloy18 x 7.5 aluminum alloy19 x 7.5 aluminum alloy  |
| Tires  | P235/65 R17 P235/60 R18P235/55 R19  |
| **EXTERIOR DIMENSIONS** |
|  | **Santa Fe Sport** | **Santa Fe** |
| Wheelbase | 106.3 in | 110.2 in.  |
| Overall length | 184.6 in | 193.1 in.  |
| Overall width | 74.0 in. | 74.2 in.  |
| Overall height (w/ roof rack) | 66.1 in. (66.5 in.) | 66.5 in. (66.9 in.) |
| Wheel Tread, front  | 64.3 / 64.1 in. (17”/19”) | 64.1/64.1 in.(18"/19") |
| Wheel Tread, rear | 64.7 / 64.5 in. (17”/19”) | 64.5/64.5 in.(18"/19") |
| **INTERIOR DIMENSIONS** |
|  | **Santa Fe Sport** | **Santa Fe** |
| Head room (w/ sunroof) | Front  | 39.6 in. (38.2 in.) | 39.6 in. (38.2 in.) |
| 2nd row | 39.1 in. (37.4 in.) | 39.4 in. (38.3 in.) |
| 3rd row | N/A | 35.7 in. (35.7 in.) |
| Leg room | Front (MAX) | 41.3 in. (44.1 in.) | 41.3 in. (44.1 in.) |
| 2nd row | 39.4 in | 41.3 in |
| 3rd row | N/A | 31.5 in |
| Shoulder room   | Front | 59.4 in. | 59.4 in. |
| 2nd row | 58.3 in | 58.6 in. |
| 3rd row | N/A | 53.9 in. |
| Hip room | Front | 56.7 in. | 56.7 in. |
| 2nd row | 55.4 in. | 55.4 in. |
| 3rd row | N/A | 44.1 in |
| SAE passenger volume | 108.0 cubic ft. | 146.6 cubic ft. |
| SAE cargo volume – Behind front seats (est.) | 71.5 cubic ft. | 80.0 cubic ft. |
| SAE cargo volume – Behind 2nd row seats (est.) | 35.4 cubic ft. | 40.9 cubic ft. |
| SAE cargo volume – Behind 3rd row seats (est.) | N/A | 13.5 cubic ft. |
| **CAPACITIES** |
|  | **Santa Fe Sport**  | **Santa Fe** |
| **2.4L** | **2.0T** | **3.3L** |
| Fuel  | 17.4 gallons | 17.4 gallons | 18.8 gallons |
| Oil  | 5.8 quarts (5.5 liter) | 5.8 quarts (5.5 liter) | 6.9 quarts (6.5 liters) |
| Coolant  | 2.7 quarts (2.55 liter) | 2.7 quarts (2.55 liter) | 4.6 quarts (4.4 liters) |
| **CURB WEIGHT** |
|  | **Santa Fe Sport**  | **Santa Fe** |
| **2.4L** | **2.0T** | **GLS** | **Limited** |
| FWD | 3,459 lbs. | 3,569 lbs. | 3,946 lbs. | 3,915 lbs. |
| AWD | 3,616 lbs. | 3,706 lbs. | 4,098 lbs. | 4,068 lbs. |
| **FUEL ECONOMY** |
|  | **Santa Fe Sport** | **Santa Fe** |
| **2.4L** | **2.0T** | **3.3L** |
| FWD A/T (EPA) |
| City | 21 mpg | 20 mpg | 18 mpg(Estimated) |
| Highway | 29 mpg | 27 mpg | 25 mpg(Estimated) |
| Combined | 24 mpg | 23 mpg | 20 mpg(Estimated) |
| AWD A/T (EPA) |
| City | 20 mpg | 19 mpg | 18 mpg(Estimated) |
| Highway | 26 mpg | 24 mpg | 24 mpg(Estimated) |
| Combined | 22 mpg | 21 mpg | 20 mpg(Estimated) |