|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **G:\Art, Photos, Logos, Movies, etc\logos\Hyundai_Chrome_Blue_Stacked.jpg** | | Hyundai Motor America 3200 Park Center Drive, Costa Mesa, CA 92867  **TEL: 714-965-3000 FAX: 714-378-1008 MEDIA WEBSITE: HyundaiNews.com**  **CORPORATE WEBSITE: HyundaiUSA.com** | | | | | NewsBureauLogo | | | | |
| **2013 Santa Fe** | | | | | | | | | |
| **ENGINE** | | | | | | | | | | | |
|  | | | **Santa Fe Sport** | | | | | | | **Santa Fe** | |
| **2.4L** | | | **2.0L Turbo** | | | | **3.3L** | |
| Type | | | 2.4L GDI  DOHC 16-valve Inline 4-cylinder | | | 2.0L Turbo GDI DOHC 16-valve Inline 4-cylinder | | | | 3.3L GDI  DOHC 24-valve V6 | |
| Materials | | | Aluminum block/aluminum cylinder heads | | | Aluminum block/aluminum cylinder heads | | | | Aluminum block/aluminum cylinder heads | |
| Bore & stroke | | | 88.0 mm x 97.0 mm | | | 86.0 mm x 86.0 mm | | | | 92.0 mm x 83.8 mm | |
| Displacement | | | 2.4L / 2,359 cc | | | 2.0 L / 1,998 cc | | | | 3.3L / 3,342 cc | |
| Horsepower | | | 190 @ 6,300 rpm | | | 264 @ 6,000 rpm | | | | 290 @ 6,400 rpm | |
| Torque | | | 181 lb-ft @ 4,250 rpm | | | 269 lb-ft @ 1,750~ 3,000 rpm | | | | 252 lb-ft @ 5,200 rpm | |
| Valves per cylinder | | | 4 | | | 4 | | | | 4 | |
| Compression Ratio | | | 11.3 | | | 9.5 | | | | 11.5 | |
| **TRANSMISSION** | | | | | | | | | | | |
| 6-speed electronic automatic | | | **Santa Fe Sport** | | | | | | | **Santa Fe** | |
| Gear ratios | | | **2.4L** | | | **2.0T** | | | | **3.3L** | |
| First | | | 4.639 | | | 4.651 | | | | 4.651 | |
| Second | | | 2.826 | | | 2.831 | | | | 2.831 | |
| Third | | | 1.841 | | | 1.842 | | | | 1.842 | |
| Fourth | | | 1,386 | | | 1.386 | | | | 1.386 | |
| Fifth | | | 1.000 | | | 1.000 | | | | 1.000 | |
| Sixth | | | 0.772 | | | 0.772 | | | | 0.772 | |
| Reverse | | | 3.385 | | | 3.393 | | | | 3.393 | |
| Final Gear Ratio | | | 3.648 | | | 3.510 | | | | 3.041 | |
| **TOWING** | | | | | | | | | | | |
|  | | | **Santa Fe Sport** | | | | | | | **Santa Fe** | |
| Towing Capacity (Trailer Weight) | | | **2.4L** | | | **2.0T** | | | | **3.3L** | |
| Without trailer brake | | | 2,000 lbs. | | | 3,500 lbs. | | | | 5,000 lbs. | |
| **SUSPENSION** | | | | | | | | | | | |
| Front | | | | | MacPherson strut with twin-tube gas filled damper and 26-mm stabilizer bar | | | | | | |
| Rear | | | | | Multi-link with gas shock absorber and (FWD 21 mm AWD 19 mm) stabilizer bar | | | | | | |
| **STEERING** | | | | | | | | | | | |
| Type | | | | | Motor Driven Power Steering (MDPS) | | | | | | |
| Overall Ratio | | | | | 15.03 : 1 | | | | | | |
| Turns, lock to lock | | | | | 2.95 | | | | | | |
| Turning circle (curb to curb) | | | | | 35.8 ft (Santa Fe Sport), 36.9 ft (Santa Fe) | | | | | | |
| **BRAKES/TIRES/WHEELS** | | | | | | | | | | | |
| Front | | | | | Ventilated single piston disc, 12.6 in. x 1.1 in. (320mm x 28mm) | | | | | | |
| Rear | | | | | Solid single piston disc, 11.9 in. X 0.4 in. (302mm x 11mm) | | | | | | |
| ABS | | | | | 4-wheel, 4-channel, 4-sensors with Electronic Brake-force Distribution (EBD) and Brake Assist | | | | | | |
| Wheels | | | | | 17 x 7.0 aluminum alloy  18 x 7.5 aluminum alloy  19 x 7.5 aluminum alloy | | | | | | |
| Tires | | | | | P235/65 R17  P235/60 R18  P235/55 R19 | | | | | | |
| **EXTERIOR DIMENSIONS** | | | | | | | | | | | |
|  | | | | | **Santa Fe Sport** | | | **Santa Fe** | | | |
| Wheelbase | | | | | 106.3 in | | | 110.2 in. | | | |
| Overall length | | | | | 184.6 in | | | 193.1 in. | | | |
| Overall width | | | | | 74.0 in. | | | 74.2 in. | | | |
| Overall height (w/ roof rack) | | | | | 66.1 in. (66.5 in.) | | | 66.5 in. (66.9 in.) | | | |
| Wheel Tread, front | | | | | 64.3 / 64.1 in. (17”/19”) | | | 64.1/64.1 in.(18"/19") | | | |
| Wheel Tread, rear | | | | | 64.7 / 64.5 in. (17”/19”) | | | 64.5/64.5 in.(18"/19") | | | |
| **INTERIOR DIMENSIONS** | | | | | | | | | | | |
|  | | | | **Santa Fe Sport** | | | | **Santa Fe** | | | |
| Head room  (w/ sunroof) | Front | | | 39.6 in. (38.2 in.) | | | | 39.6 in. (38.2 in.) | | | |
| 2nd row | | | 39.1 in. (37.4 in.) | | | | 39.4 in. (38.3 in.) | | | |
| 3rd row | | | N/A | | | | 35.7 in. (35.7 in.) | | | |
| Leg room | Front (MAX) | | | 41.3 in. (44.1 in.) | | | | 41.3 in. (44.1 in.) | | | |
| 2nd row | | | 39.4 in | | | | 41.3 in | | | |
| 3rd row | | | N/A | | | | 31.5 in | | | |
| Shoulder room | Front | | | 59.4 in. | | | | 59.4 in. | | | |
| 2nd row | | | 58.3 in | | | | 58.6 in. | | | |
| 3rd row | | | N/A | | | | 53.9 in. | | | |
| Hip room | Front | | | 56.7 in. | | | | 56.7 in. | | | |
| 2nd row | | | 55.4 in. | | | | 55.4 in. | | | |
| 3rd row | | | N/A | | | | 44.1 in | | | |
| SAE passenger volume | | | | 108.0 cubic ft. | | | | 146.6 cubic ft. | | | |
| SAE cargo volume – Behind front seats (est.) | | | | 71.5 cubic ft. | | | | 80.0 cubic ft. | | | |
| SAE cargo volume – Behind 2nd row seats (est.) | | | | 35.4 cubic ft. | | | | 40.9 cubic ft. | | | |
| SAE cargo volume – Behind 3rd row seats (est.) | | | | N/A | | | | 13.5 cubic ft. | | | |
| **CAPACITIES** | | | | | | | | | | | |
|  | | | | **Santa Fe Sport** | | | | | **Santa Fe** | | |
| **2.4L** | | **2.0T** | | | **3.3L** | | |
| Fuel | | | | 17.4 gallons | | 17.4 gallons | | | 18.8 gallons | | |
| Oil | | | | 5.8 quarts  (5.5 liter) | | 5.8 quarts  (5.5 liter) | | | 6.9 quarts  (6.5 liters) | | |
| Coolant | | | | 2.7 quarts  (2.55 liter) | | 2.7 quarts  (2.55 liter) | | | 4.6 quarts  (4.4 liters) | | |
| **CURB WEIGHT** | | | | | | | | | | | |
|  | | | | **Santa Fe Sport** | | | | | **Santa Fe** | | |
| **2.4L** | | **2.0T** | | | **GLS** | | **Limited** |
| FWD | | | | 3,459 lbs. | | 3,569 lbs. | | | 3,946 lbs. | | 3,915 lbs. |
| AWD | | | | 3,616 lbs. | | 3,706 lbs. | | | 4,098 lbs. | | 4,068 lbs. |
| **FUEL ECONOMY** | | | | | | | | | | | |
|  | | | | **Santa Fe Sport** | | | | | **Santa Fe** | | |
| **2.4L** | | **2.0T** | | | **3.3L** | | |
| FWD A/T (EPA) | | | | | | | | | | | |
| City | | | | 21 mpg | | 20 mpg | | | 18 mpg  (Estimated) | | |
| Highway | | | | 29 mpg | | 27 mpg | | | 25 mpg  (Estimated) | | |
| Combined | | | | 24 mpg | | 23 mpg | | | 20 mpg  (Estimated) | | |
| AWD A/T (EPA) | | | | | | | | | | | |
| City | | | | 20 mpg | | 19 mpg | | | 18 mpg  (Estimated) | | |
| Highway | | | | 26 mpg | | 24 mpg | | | 24 mpg  (Estimated) | | |
| Combined | | | | 22 mpg | | 21 mpg | | | 20 mpg  (Estimated) | | |